What does STS store exactly?

What does LDS do.. and how does it work?

What does masking the bits do?

TFLG1, 4 );

TMSK1, 4 );