What does STS store exactly?

What does LDS do.. and how does it work?

What does masking the bits:

TFLG1, 4 );

TMSK1, 4 );

do?

What bits should I mask in order to generate an interrupt... How do I find this out in the manual?

TFLG1, 4 );

TMSK1, 4 );